IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2023-05-03T16:23:43"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Default UI"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "CONDENSINOX 50_kW" | object type "CONDENSINOX 50_kW" | names: "Condensinox-Cadenso - depuis 2021-02_FR_D:CONDENSINOX 50_kW:9787" | material: materials ("Par défaut", "BLEUGUILLOT", "Translucide") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCBUILDINGELEMENTPROXYTYPE "CONDENSINOX 50_kW" | 1 occurrence | material: materials ("Par défaut", "BLEUGUILLOT", "Translucide") | property sets: Data, Dimensions, Electrical, General, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "CONDENSINOX 50_kW" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Atlantic Solutions Chaufferie" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 3.94610151035497 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.532455284655285 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Alimentation gaz = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Decalage_lateral_purgeur = 269. (IFCLENGTHMEASURE) [MILLI METRE]
    Départ eau chaude = 42.4 (IFCLENGTHMEASURE) [MILLI METRE]
    E = 58. (IFCLENGTHMEASURE) [MILLI METRE]
    Entree air frais = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Evacuation condensats = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    F = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur hors options = 1494. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_Totale = 1494. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_afficheur_HMI_IMH = 1158. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_capot = 183.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_depart = 406. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_depart_cheminee = 1449. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_evacuation_condensats = 114. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_mini_pieds = 19.9999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_piquage_gaz = 1354. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_retour_chaud = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur_retour_froid = 336. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur hors options = 595. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids à vide (kg) = "140" (IFCTEXT)
    Position_laterale_logo_atl = 550. (IFCLENGTHMEASURE) [MILLI METRE]
    Position_laterale_piquage_gaz = 205. (IFCLENGTHMEASURE) [MILLI METRE]
    Position_laterale_piquages = 76. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur habillage = 670. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur hors options = 708. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur_piquage_gaz = 46. (IFCLENGTHMEASURE) [MILLI METRE]
    Retour chaud = 42.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Retour eau froide = 42.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sortie fumee = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume d'eau (L) = "88" (IFCTEXT)
    dimensions d'installation = "1750 x 995 x 1970" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "864865" (IFCTEXT)
    BC_OBJECT_ID = "286580" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "708336" (IFCTEXT)
    Code Article = "041812/041548" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Copyright = "" (IFCTEXT)
    Description = "Chaudière sol gaz à condensation en inox 60 kW" (IFCTEXT)
    Famille = "Chaudière collective sol gaz" (IFCTEXT)
    Lien page produit = "" (IFCTEXT)
    Manufacturer = "Atlantic Solutions Chaufferie" (IFCTEXT)
    Model = "Condensinox 50" (IFCTEXT)
    Numéro d'article commerce international (NACI) = "" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Référence = "CONDENSINOX 50_kW" (IFCTEXT)
    Type Name = "CONDENSINOX 50_kW" (IFCTEXT)
    Type de l'Objet = "" (IFCTEXT)
    URL = "https://www.atlantic-solutions-chaufferie.fr/" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Hydronic Supply,Hydronic Return,Other,Hydronic Supply,Other" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Condensinox-Cadenso - depuis 2021-02_FR_D: CONDENSINOX 50_kW" (IFCLABEL)
    Family and Type = "Condensinox-Cadenso - depuis 2021-02_FR_D: CONDENSINOX 50_kW" (IFCLABEL)
    Type = "Condensinox-Cadenso - depuis 2021-02_FR_D: CONDENSINOX 50_kW" (IFCLABEL)
    Type Id = "Condensinox-Cadenso - depuis 2021-02_FR_D: CONDENSINOX 50_kW" (IFCLABEL)
    Zone de maintenance = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Concepteurs = "Bim Conseil Formation / HMT International" (IFCTEXT)
    Distance _Dentretient_LateraleA = 199.999999999997 (IFCLENGTHMEASURE) [MILLI METRE]
    Distance-Dentretien_haut = 1750. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance_Dentretien_ArriereC = 200.000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Distance_Dentretien_avant = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Evac a = FALSE (IFCBOOLEAN)
    Evac b = FALSE (IFCBOOLEAN)
    Family Name = "Condensinox-Cadenso - depuis 2021-02_FR_D" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Data | properties | on 1 type object
    Classe Nox = "6" (IFCTEXT)
    Etiquette énergie (disponible sur nos sites) = "https://www.atlantic-solutions-chaufferie.fr/chaudieres-gaz/chaudieres-gaz-sol-condensation/condensinox" (IFCTEXT)
    Lien données RT (Edibatec) = "http://www.edibatec.org/consult/fiche_produit.php?codeEdi=CHAUDRSGUI06005" (IFCTEXT)
    Lien fiche Pep = "http://register.pep-ecopassport.org/fileadmin/tx_pepmanagement/user_upload/SCGA-00050-V01.01-FR_pdfpep_02.pdf" (IFCTEXT)
    Matériau corps de chauffe = "Acier inoxydable" (IFCTEXT)
    Nombre piquages = "2 ou 3" (IFCTEXT)
    Pression d'alimentation gaz naturel (mbar) = "20" (IFCTEXT)
    Pression d'alimentation propane (mbar) = "37" (IFCTEXT)
    Pression de service (bar) = "4" (IFCTEXT)
    Puissance utile nominale à régime 50/30 °C (kW) = "54.1" (IFCTEXT)
    Puissance utile nominale à régime 80/60 °C (kW) = "49.9" (IFCTEXT)
    Période de vente du produit (depuis le / à partir de) = "" (IFCTEXT)
    Raccordement fumées = "Cheminée (B23/B23p) et Ventouse (C13/C33/C53)" (IFCTEXT)
    Taux de modulation (%) = "20" (IFCTEXT)
    Type d'énergie = "Gaz naturel ou Propane" (IFCTEXT)
    température de consigne départ maximale (°C) = "80" (IFCTEXT)
  Electrical | properties | on 1 type object
    Fréquence = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Indice de protection (IP) = "IP20" (IFCTEXT)
    Puissance nominale absorbée = 142. (IFCPOWERMEASURE) [WATT]
    Réseau (mono/tri) = "Monophasé" (IFCTEXT)
    Tension d'alimentation = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  General | properties | on 1 type object
    Garantie pièces détachées (ans) = "2" (IFCTEXT)
    Garantie produit (ans) = "3" (IFCTEXT)
    Lien pièces détachées = "" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Materiau_porte_tableau_commande = "tole_grise_metallisee" (IFCLABEL)
    Materiau_socle = "acier noir" (IFCLABEL)