IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "26fcc3d7-afa8-47ff-875d-f00b5d9310cd.ifc"
Time stamp: "2017-12-13T10:43:23"
Author: "BouwConnect Bibliotheek"
Organization: "De Twee Snoeken"
Preprocessor: "IFC Engine DLL"
Originating system: "BouwConnect Bibliotheek"
Authorization: "De Twee Snoeken"
Application: "BouwConnect Bibliotheek" version "1.0" identifier "BouwConnect Bibliotheek" by Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek"

People and organizations
  Person "webapp.bcb" of Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek"
  Owner history of Person "webapp.bcb" of Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek" | application "BouwConnect Bibliotheek" version "1.0" identifier "BouwConnect Bibliotheek" by Organization "BouwConnect Bibliotheek" description "BouwConnect Bibliotheek" | change ADDED | created 1513161803 (2017-12-13T10:43:23Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "cv ketel HR ketel ATAG - Q-Serie Q38S"
  IFCSITE "Kavel" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.
    IFCBUILDING "Gebouw" | postal address: "Gebouw"
      IFCBUILDINGSTOREY "Bouwlaag" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | names: "cv ketel HR ketel ATAG - Q-Serie Q38S" | material: "metaal" | property sets: Pset_Data

Property sets
  Pset_Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    HR-label = "107" (IFCTEXT)
    Hyperlink = "http://bcb-online.nl/?WUID=AgAAACOAcyYCAAAAfVgBAAWTZwAAzPoAALtzAABfOQEAY08BAAEAEAABAQAAAAEAAADvrgAABXC5AABkMAAAxqcAAKOtAADp2AAAAAA)" (IFCTEXT)
    STABU2 = "60.51.11" (IFCTEXT)
    WUID = "AgAAACOAcyYCAAAAfVgBAAWTZwAAzPoAALtzAABfOQEAY08BAAEAEAABAQAAAAEAAADvrgAABXC5AABkMAAAxqcAAKOtAADp2AAAAAA)" (IFCTEXT)
    artikelnummer = "SA5BB10H" (IFCTEXT)
    breedte = "500" (IFCTEXT) [mm (context dependent)]
    diepte = "385" (IFCTEXT) [mm (context dependent)]
    eenheid = "st" (IFCTEXT)
    energiedrager = "gas" (IFCTEXT)
    gaskeur certificaat = "False" (IFCTEXT)
    gelijkwaardigheidsverklaring = "True" (IFCTEXT)
    gewicht per st = "53" (IFCTEXT) [kg/st (context dependent)]
    hoofdmateriaal = "metaal" (IFCTEXT)
    hoogte = "680" (IFCTEXT) [mm (context dependent)]
    kenmerkende grondstof = "metaal" (IFCTEXT)
    merk = "ATAG" (IFCTEXT)
    nominaal vermogen = "38" (IFCTEXT) [kW (context dependent)]
    ondergrens van de modulatie = "0,19" (IFCTEXT)
    opwekkingsrendement verwarming = "0,975" (IFCTEXT)
    opwekkingsrendement verwarming reken = "0,975" (IFCTEXT)
    prijspeil = "1-9-2013 0:00:00" (IFCTEXT)
    rapporten = "DhObject.DhExterneReferentieLijst" (IFCTEXT)
    serie = "Q-Serie" (IFCTEXT)
    type = "Q38S" (IFCTEXT)
    vloeistof inhoud = "5" (IFCTEXT) [l (context dependent)]